**Test Platform Cable User Manual**

**1. Wiring Connection**

****

Pic. 1 Cables & adapters wiring connection diagram

**二、钥匙放置**

**2. Key Position**

****

Pic. 2 Emergency-Start coil position

**Put the key marked with red (see above pic.2) on the coil.**

**三、START/STOP按键操作**

**3. START/STOP button operation**



D1为START/STOP按键状态指示灯, 接上电源, 指示灯点亮。

D2为发动机自动启停装置( MSA ) 状态指示灯。默认熄灭。

D3为电门状态指示灯, 可代替仪表显示电门状态。电门打开时, 指示灯亮; 电门关闭时, 指示灯灭。

D1: START/STOP button’s indicator- light on when the power supply is connected

D2: Automatic stop and start function (MSA) indicator- default status: light off

D3: Engine fire shutoff switch’s indicator (to replace the dashboard and display the status of the engine fire shutoff switch)- light on when the switch is turned on and light off when the engine is turned off

**打开电门操作:**

将工作钥匙放在线圈上, 按下按键, 电门状态指示灯 ( D3 ) 点亮。若指示灯不亮, 可稍等3~5秒再按一次。

How to turn on the engine fire shutoff switch:

Put the working key on the coil;

Press the button;

Engine fire shutoff switch indicator (D3) lights on;

(If the indicator fails to light on, wait for 3-5 seconds and press it again)

**关闭电门操作:**

 连按三次按键, 指示灯( D3 )熄灭, 则电门关闭。

How to turn off the engine fire shutoff switch:

Press it continuously for 3 times;

Engine fire shutoff switch indicator (D3) lights off- engine fire shutoff switch is turned off