**Important Notes on Replacement of New Supplier’s TP Screen on MaxiSys Tablets**

1. **Part Number of new TP screen Involved**

501003930 MS906

501003932 MS906BT

501004169 MS908

501003923 MS908S


Note: The above new TP screen is provided by a new supplier, which will be used for TP replacement of the above models.

1. **Preparations:**
2. **Update operating system to the latest version first**


E.g. Maxisys 906 V03.46.00, Maxisys906BT V03.31.00 , MY908 V03.41.00

If the MaxiSys was out of update period, please use reflashing program(sent via Wetransfer) to update it to the free version.


1. **Remove Resistance**
2. Remove R289 Resistance for MY908




1. Remove R375 Resistance for MY906/MY906BT



1. **Remove specific buttons for MY906,MY906BT,MY906TS**
2. Remove J11, J12 buttons(as showed below) for MY06BT, MY906TS



2. Remove J11, J12 buttons (as showed below) for MY906



1. **Pasting way of TP for MY906,MY906BT,MY906TS**

TP plate should be pasted parallelly with the magnesium alloy stent.



**TP钢片与**

**镁合金支架**

**平齐粘贴**