|  |
| --- |
| **FLY OBD Terminator Support car List** |
| 1. **ALL Honda**; |
| 2. **ALL Ford**; |
| 3. **ALL Mazda**; |
| 4. **ALL LandRover**; |
| 5. **ALL Jaguar** ; |
| 6. **ALL Toyota and Lexus** ; |
| 7. **A4/A5/Q5 2007+ Generation 5 Immobilizer**;（   1.Read BCM2 Immobilizer Data By OBDII;   2.Generate dealers keys and key learning;   3.Open/close Immobilizer Horn;   4.Recover Emergency data(Data recovery and wake up in the process of reading immobilizer data failure cases);   5.Check the new PCF7945AC (HitagExt VAG);   6.Load decode file (Can generate dealer key and learning key);   7.Load PFLASH and DFLASH file (Can generate dealer key and learning key);   ）; |
| 8. **A6/A7/A8/VW Touareg Generation 5 Immobilizer**;（   1.Read BCM2 Immobilizer Data By OBDII;   2.Generate dealers keys and key learning;   3.Open/close Immobilizer Horn;   4.Recover Emergency data(Data recovery and wake up in the process of reading immobilizer data failure cases);   5.Check the new PCF7945AC (HitagExt VAG);   6.Load decode file (Can generate dealer key and learning key);   ）; |
| 9. **PIN Calculator Functions:**（   1.Nissan 20-digit and 5-digit PIN Calculator;   2.JLR SDD Coded Access Password Calculator;   3.Ford and Mazda Incode Calculator(Include 6-digit,12-digit or 16-digit Outcode);   4.Honda Password Calculator(Include First Password, Second Password, HIM Unlock Password and 4-digit PCM Password    ); |
| 10. **Reset of Toyota/Lexus/Subaru Smart Keys**（   1.Reset of Toyota/Lexus/Subaru Smart Keys 40,80,128 bit;   ）; |
| 11. **VAG Generation 4 Immobilizer，NEC Dashboard 95320**;（   1.Automatically recognize VAG Generation 4 NEC 95320 Dashboard;   2.Add VAG Generation 4 NEC 95320 Dashboard key directly;   3.Read VAG Generation 4 NEC 95320 Dashboard Immobilizer data;   4.Modify VAG Generation 4 NEC 95320 Dashboard Immobilizer data;   5.Read and save VAG Generation 4 NEC 95320 Dashboard configuration data;   ）； |
| 12. **VAG Generation 4 Immobilizer, NEC Dashboard 24C32**; |
| 13. **JLR SDD Coded Access Password for Locked Functions**;    **1.Jaguar:**      CCF EDITOR      ODO APP (X150)      ODO APP (X250)      ODO APP (X351)      SOFTWARE DOWNLOAD      VID BLOCK EDITOR      VIN BYPASS      RECOVER KEYS (X351) ;   **2.Land Rover:**      CCF EDITOR      ODO APP (L316))      ERASE KEYS (L322)      ODO APP (L322)      RECOVER KEYS (L322)      OPTION 8      SOFTWARE DOWNLOAD      VEHICLE UPDATE (Only Taiwan models) |
|  |