**Remote Tester Frequency/Infrared IR RT100**

RF100 Remote Tester Radio Frequency(RF) Infrared(IR) can detect frequency as well as infrared working or not.

**Frequency Test Range:**

■300Mhz-320Mhz

■434Mhz

■868Mhz

**Way to Test Frequency:**

■Put the remote control close to the device

■Press any button on the remote control

■The lit indicator shows the frequency

**Way to Test Infrared Working or Not:**

The infrared works well if the indicator lits up after pressing the key button, otherwises, it is in malfunction